**ACKNOWLEDGEMENT**

We express our sincere thanks to **Sir.Suhil Ahmed** principal GPT Kampli for providing all the required facilities for completion of our project.

We express our sincere gratitude to our Head of the department **Ms.Shabana B.S** in Computer science and Engineering department for her encouragement, moral support, for providing all the required facilities for the smooth functioning of the project.

We are also grateful and express our sincere thanks to my project guide **Ms.Shabana B.S**

Lecturer in computer science & Engineering department, for giving the all-possible support,

Guidelines and her kind encouragement in completion of the project.

Last but not the least, we would like to thank the Teaching & Non-Teaching Staff of

Computer science Engineering department, we would like to thank one and all who have

Helped us during the course if this project.

**ABSTRACT**

Remote Bluetooth this useful for controlling the Pc via Bluetooth connectivity within the limited distance. If we have this application in our mobile, no need Mouse. Therefore without Mouse we can Control Pc with the help of Bluetooth connectivity which is the main use of this application. The major defect of this device is, if both of the cells are out of Bluetooth range then it’s difficult to get connection between both the smart phone and pc.

Remote Bluetooth has two parts:

* + 1. Android
    2. Java

In this project the client side android and server side is the java. Client is the machine which can connect to Server. Server is the machine which handles the particular client. By this process we can easily Smart phone connect to the Pc. First active Bluetooth both in client and server device and after that process client & server gets connected with each other.

In this way users gets connected the Pc, but there is one limitation in this application. Server is able to find all the active Bluetooth devices but it can connect with only one at a time. There is no way to connect simultaneously with all smart phone. Here one more drawback is for controlling with voice internet connection needed. We can only controlling Pc within the Bluetooth range which is limited up to certain specific distance. The main purpose of this application is controlling the Pc